Canon UFR II Printer Driver Version 30.10 for Microsoft Windows
Before using this software, please be sure to read the CANON SOFTWARE LICENSE AGREEMENT displayed during installation. You can also view the CANON SOFTWARE LICENSE AGREEMENT (EULA.rtf) stored in the [misc] in the accompanying CD-ROM or downloaded driver folder.
This file contains supplemental information to help you install and use this printer driver with Microsoft Windows.
As with most software and hardware products, some information is made available after the development of the manual. Updated information regarding this driver software is provided in this README file. If you require additional assistance, please contact your local Canon company.
Microsoft, Windows, and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.
Other product and company names herein may be the trademarks of their respective owners.
CONTENTS
Overview
System Requirements
Accessing the Properties Dialog Box
Accessing Help Information
Cautions, Limitations and Restrictions
Overview
This printer driver allows you to print documents from any Windows application to your printer.
NOTE
This driver supports the Canon Driver Configuration Tool. You can change the factory default settings of the printer driver to create customized driver sets using the Canon Driver Configuration Tool. For detailed information about this utility, refer to the Canon Driver Configuration Tool User's Guide.
System Requirements
This printer driver can be used in the following environments:
Operating Systems
Windows Vista
Windows 7
Windows 8
Windows 8.1
Windows 10
Windows Server 2008
Windows Server 2008 R2
Windows Server 2012
Windows Server 2012 R2
Windows Server 2016
Server-based Computing Environment
Server Operating Systems
Windows Server 2008
Windows Server 2008 R2
Windows Server 2012
Windows Server 2012 R2
Windows Server 2016
Server Components
Citrix Presentation Server 4.5
Citrix XenApp 5.0
Citrix XenApp 6.0
Citrix XenApp 6.5
Citrix XenApp 7.5
Citrix XenApp 7.6
Citrix XenApp 7.7
Citrix XenApp 7.8
Citrix XenApp 7.9
Citrix XenApp 7.11
Citrix XenApp 7.12
Citrix XenDesktop 4.0
Citrix XenDesktop 5.0
Citrix XenDesktop 5.5
Citrix XenDesktop 5.6
Citrix XenDesktop 7.0
Citrix XenDesktop 7.1
Citrix XenDesktop 7.5
Citrix XenDesktop 7.6
Citrix XenDesktop 7.7
Citrix XenDesktop 7.8
Citrix XenDesktop 7.9
Citrix XenDesktop 7.11
Citrix XenDesktop 7.12
VMware vSphere 4
VMware vSphere 5
VMware vSphere 5.1
VMware vSphere 5.5
Microsoft Application Virtualization (App-V)
Remote Desktop Service on Windows Server 2012 R2
TS-RemoteApp on Windows Server 2008
Cluster Server
Microsoft Windows Server 2008 Enterprise/Datacenter Edition
Microsoft Windows Server 2008 R2 Enterprise/Datacenter Edition
Microsoft Windows Server 2012
Microsoft Windows Server 2012 R2
Microsoft Windows Server 2016
Computer
Any computer which runs the above operating system software properly.
However, at least one of the following output ports is required:
- network interface
- USB port
The network interface is recommended for the highest quality printing throughput.
Accessing the Properties Dialog Box
The Properties dialog box contains several sheets that allow you to setup and control your printer. To access the Properties dialog box, use one of the following procedures:
To access from the Desktop:
1. Display [Devices and Printers] from the [Control Panel] of Windows.
2.Right-click the printer icon for your printer in the Printers folder, and then click [Properties] or [Printer properties] to open the [Printer properties] dialog box, or click [Printing Preferences] to open the [Document Properties] dialog box (or [Printing Preferences] dialog box).
To access from within an application:
1.Click the [Print] command to display the [Print] dialog box.
2.Select your printer name from the drop-down list box, and then click the [Properties] button.
Accessing Help Information
From the Properties dialog box, you can click the [Help] button to display the information about the printer driver.
Cautions, Limitations and Restrictions
If you print a document that has an odd number of pages as a two-sided document from an application, the application may automatically insert a blank page to bring the number of pages up to an even number. When this happens, the blank page inserted by the application is counted up in the same way as a printed page.
To register the custom paper size you want to use, access the [Document Properties] dialog box from the Printers folder with Administrator privileges, and then specify the paper size in the [Custom Paper Size Settings] dialog box which is displayed by clicking the [Custom Paper Size] button in the [Page Setup] sheet.
If you are using Server Core in your Windows Server operating system, you cannot use the printer driver installer. Use the installation function of the operating system to install the printer driver.
You cannot install the driver with the installer. Use the installation options of Windows.
Some print options are not available under local environment or Windows Remote Desktop environment.
If you are using a printer that supports 2-sided printing, the default setting is 2-sided printing.
When using the driver in a USB/WSD connection environment, you cannot use the Get Device Status function, Department ID Management function, and User Authentication function.

Copyright Canon Inc. 2003